# Computational Methods for Multiphase Flows in Porous Media

Displacement mechanisms of thermal methods:

1. Reduction of crude viscosity with increasing temperature (most important)
2. Change of relative permeabilities for greater oil mobility
3. Vaporization of connate water and of a portion of crudes for miscible displacement of light components
4. High temperatures of fluids and rock to maintain high reservoir pressure.